{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":15},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":10,"rows_kept":20,"merged":[[0,0,0,9],[1,1,1,2],[2,1,3,1],[5,1,5,2],[6,1,6,2],[17,1,17,2],[18,1,18,2],[19,1,19,7]],"flags":["formulas_cached_only"]}
["技术参数要求及明细报价表"]
["序号","产品名称及型号",null,"材质(技术参数)","尺寸cm","数量","单位","单价","小计","备注"]
[1,null,"卡通雕塑","玻璃钢开模定制","高160X60\n高130X60",3,"座"]
[2,null,"主题文字及底座","镀锌板烤漆","高50X450X100",1,"套"]
[3,null,"电器火灾演示实验台\nV1.0 ","实验台配备大功率用电器，当系统启动小功率用电器时，线路正常供电；当系统启动大功率用电器时，测试电线开始发热，并逐渐燃烧，直到烧断；当更换合适的导线后，同时开启大、小功率用电器时，空气开关过载并发生跳闸现象；该设备在演示过程中，电路的电压、电流均通过数显设备实施显示演示过程的数值",null,4,"台"]
[4,"电器火灾试验台",null,"定制+万向轮","70X70X75",4,"组"]
[5,"电器火灾成应设备介绍",null,"亚克力UV","50X65",4,"块"]
[6,null,"试验台","钢木实验台，带右侧水槽","高80X75X250",1,"套"]
[7,null,"试验台造型","PVC裱亚克力UV-雕刻造型","70X250",1,"套"]
[8,null,"消防之窗宣传栏","方钢、镀锌板烤漆，开启式画框","270X600",1,"套"]
[9,null,"消防标识翻版宣传栏","方钢、镀锌板烤漆，开启式画框","265X580",1,"套"]
[10,null,"消防安全单窗口宣传栏","方钢、镀锌板烤漆，开启式画框","240X265",2,"套"]
[11,null,"楼顶主题字","烤漆字","80X80",8,"个"]
[12,null,"教室造型黑板报","120X240cm成品黑板，\nPVC裱亚克力UV-雕刻造型","240X510",1,"套"]
[13,null,"教室制度牌","开启式画框+PVC画面","60X90",3,"套"]
[14,null,"教室消防安全知识","PVC裱亚克力UV-雕刻造型","60X180",6,"组"]
[15,null,"走廊墙面消防知识","PVC裱亚克力UV-雕刻造型","150X420X2套\n180X275\n",3,"套"]
[16,"水电及消防设施改造",null,"教室通水、裸露电缆处理、线桥处理、消火栓及管道装饰改造、柜、橱、防火门更换（4樘）等",null,1,"项"]
[17,"运输、安装及辅材",{"$nulls":3},1,"项"]
[18,"合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}